Specification
POE

A. General
i.	The POE (“Power over Ethernet Switch”) shall be a solid-state device specifically designed as an unmanaged Power over Ethernet network switch.
ii.	There shall be visual indicators on the Power over Ethernet Switch showing status of the Power over Ethernet Switch and its interfaces.
iii.	The Power over Ethernet switch shall support 4 PoE ports.
iv.	The Power over Ethernet switch shall support 2 non-PoE ports.
v.	All Ethernet ports of the Power over Ethernet switch shall support automatic MDI/MDI-X configuration.
vi.	The Power over Ethernet Switch shall be provided with a 5 year manufacturer warranty.

B. Physical
i.	Enclosure and mounting shall comply with DIN43880 and EN60715(35/7.5) respectively.
ii.	The unit shall be a 6 unit DIN enclosure (107.5mm x 90.0mm x 58.0mm).
iii.	The unit shall be entirely solid-state with no moving parts or fans.
iv.	The unit shall operate in a temperature range from 0°C to 50°C (32°F to 122°F).
v.	The unit shall be CE compliant.
vi.	The unit shall be ETL/cETL listed.

C. Electrical
i.	The Power over Ethernet Switch shall be designed to support the following wire terminations (Camden Electronics CTB9208 5.08mm plug-in rising clamp terminals):
a.	3-pin 48V DC Power
and the plug-in rising clamp terminals shall be provided.
ii.	In addition there shall be the following standard connectors:
a.	RJ45 socket for 10/100Base-TX Ethernet (2).
b.	RJ45 socket for 10/100Base-TX Ethernet (IEEE 802.3af/IEEE802.3at) (4).